Actions

Fisa Project - Accessories |  |  |  |
Accessory/Position Type | Default Connections (Connections are made only if the accessory is a descendant to a position) | Automatic Program (Activations are made only if the connection is found and the Action property is correct) |  |  |  |
Output Action | Input Action (1 second or user defined response time) | Default Response Object | Activation when basket enters | Inactivation when basket exits | Special activation/inactivation Feedbacks are tested if the activation of an accessory finds an input connection with its Action property = Feedback |  |  |  |
Agitation | Activation *4 | Stopped Position | X | TL/OL *3 | OH *1 | Stop on Put/Take *2 |  |  |  |
Ultrasound (user choice) | Activation | Feedback (inversed) |  | Shut off before opening lid *2 Restore other positions after closing lids |  |  |  |
Infrared (user choice) | Activation | Feedback (inversed) |  |  |  |  |  |
User Accessory | Activation |  |  |  |  |  |  |
Electrovalve | Activation |  |  |  |  |  |  |
Pump | Activation |  |  | If the Action is Inactivation, the pump will be stopped when a basket enters the parent position. The pump is started in Prg 65 |  |  |  |
Skim Ramp | Activation | Feedback |  | OL | OH | Activate 10 s before Take |  |  |  |
Lid, Internal Lid | Open, Close *5 | Opened, Closed | XXXX |  |  | Open/Close |  |  |  |
Door | Access Permission | Closed |  |  |  | Loading/Unloading |  |  |  |
Conveyor Motor | Activation | Detected Loading Full |  |  |  | Loading/Unloading |  |  |  |
Loading Unloading |  | Detected Basket |  |  |  | For multiple loadings an input is defined on the parent of the loadings |  |  |  |
Chain and Oven Chain motor | Activation | Step Not Reached (common) | X |  |  | Simulation activates basket detector for first position on [P] and deactivates it on [S] and deactivates basket detector for conveyor end on [T] |  |  |  |
Chain and Oven extreme detectors | Detected Basket (common) + Detected basket conveyor end (local) |  |  |  |  |  |
External Liftout | Upstroke Downstroke | Cycle Ended | XX |  |  |  |  |  |  |
Lamp |  |  |  |  |  | User connection |  |  |  |
*1 Check for common connections in other positions before deactivating |  |  |  |  |  |
*2 No consideration is taken to other positions in these circumstances |  |  |  |  |  |
*3 OL is used when the output is connected to accessories belonging to other positions. |  |  |  |
*4 Consecutive Agitations (up to 4) are connectected to the same output. |  |  |  |  |  |
*5 If the next movement after taking a basket is to put a basket into the take position then leave the lid open. Exception is made if the origin is Loading or Transfer Position |  |  |  |
Output Actions |  | Input Actions |  |  |  |
Activation, Inactivation, Opening, Closing, Upstroke, Downstroke, Chain Motor, Access Permission, Connection to Input |  | Detected Basket, Detected Loading Full, Detected Basket Conveyor End, Feedback, Feedback (inversed), Opened, Closed, Cycle Ended, Step Not Reached, Stopped Position, Detected Basket on any Multiple Loadings, Oven is not Empty, Connection from Output |  |  |  |