Alarmmeldungen |

Anzeigen
Alarmoptionen
When is an alarm triggered?
If the object of the alarm is a descendant to a position:
If the object of the alarm is not a descendant to a position:
Visual indication
Alarm Arten

Alarms can be

- Freigabe (the user has acknowledged the alarm by clicking in the box)
und /oder
- Zurückgesetzt (der Instrumentwert ist wieder gut geworden, oder der Alarmzustand kann nicht zurückgestellt werden)

Alarms that have been Resetted and Acknowledged will dispappear from the list.

Anzeigen

You can resize and reorder the colums by drag and drop operations on the column headers.
You can sort the list by clicking on a column header.

Alarmoptionen

If you save and clear an Alarm, it will reapperar as a new alarm if the instrument value or the condition for the alarm has not become good.

When is an alarm triggered?

- An instrument reports an offrange value
- A maintenance prewarns
- A maintenance becomes due
- Robot Arm blocked or collision with another robot - Siehe Bediener Kurzhilfe
- Alarm activation by Robot Parameter ax, Ax, A0 - Siehe Meldungen mit Parametern vom Roboter Fisa

If the object of the alarm is a descendant to a position:

A basket present or a basket put in that position be marked with Remark.
If the object of the alarm is not a descendant to a position:

All baskets present in positions being descendants to the object will be marked with Remark.

To avoid having all baskets marked by an object at Installation level, uncheck the following submenu:
Mark Baskets for Global Alarms
Sie finden dies unter dem menü Alarm-Meldungen
Visual indication

| Ein markierter Korb ändert seine Farbe in grell rot. |

Siehe auch Korb-Farbe und Eigenschaft
Alarm Arten

- Grundsätzlich - Alarm activation by Robot Parameter - A0
- Vorwarnung - Wartung
- Überfällig - Wartung
- Überschreiten - Instrument
- Ungenügend - Instrument
- Kein Wert - Instrument
- Maximum process residence time in position exceeded - Korb
- Minimale ProzeßVerweilzeit in der Position nicht respektiert - Korb
- Ausgang - Alarm activation by Robot Parameter - Ax: x = 1 - 64
- Position - Alarm activation by Robot Parameter - ax: x = 1 - 65
- Mißlugen - Alarm activation by Robot Parameter - Ax: x = 1 - 64
- Blockierter Arm - Alarm activation by Robot Programming Unit