Default Connections

Contents
Default Connections

The following connections are automatically created using available outputs and inputs when:

- Creating a New Installation
- After structure modifications, clicking on the Program menu and submenu Default Connections of Outputs and Inputs + Response Objects

  Accessory | Output Action | Response Object | Input Action | Equipment Item
  Ultrasound Infrared | Activation | - | US/IR Failed | Ultrasound Infrared
  - | - | - | Detected Basket | Loading Unloading
  Door Loading Unloading | Access Permission | - | Closed | Door Loading Unloading
  Conveyor Motor Loading Unloading | Activation | - | Detected Loading Full | Loading Unloading
  Pump Agitation | Activation | Parameters for Response Object | - | -
  Lid Internal Lid | Opening | Time for response = User Inverted Response = No Immediate Response = No Response for OL = Yes Response for OH = Yes | Opened | Lid Internal Lid
  Lid Internal Lid | Closing | Time for response = User Inverted Response = No Immediate Response = No Response for OL = Yes Response for OH = Yes | Closed | Lid Internal Lid
  External Liftout | Upstroke | Time for response = User Inverted Response = No Immediate Response = No Response for OL = Yes Response for OH = Yes | Cycle Ended | External Liftout
  External Liftout | Downstroke | Time for response = 1 Second Inverted Response = No Immediate Response = No Response for OL = Yes Response for OH = Yes | Cycle Ended | External Liftout
  Chain Motor | Chain Motor | Time for response = User Inverted Response = Yes Immediate Response = No Response for OL = Yes Response for OH = No | Step Not Reached | Chain Motor

  Standard Actions when connecting Outputs

  | Activation Opening Closing Upstroke Downstroke Chain Motor Access Permission Connection to Input

  Standard Actions when connecting Inputs

  | Detected Basket Detected Loading Full Detected Basket Conveyor End Feedback Feedback (inversed) Opened Closed Cycle Ended Step Not Reached Stopped Position Detected Basket on any Multiple Loadings Oven is not Empty Connection from Output