Alarms Report

Contents

Alarms can be

- Acknowledged (the user has acknowledged the alarm by clicking in the box)
and/or
- Resetted (the instrument value has become good again or the alarm condition cannot be undone)

Alarms that have been Resetted and Acknowledged will dispappear from the list.

Display

You can resize and reorder the colums by drag and drop operations on the column headers.
You can sort the list by clicking on a column header.

Alarms Options

If you save and clear an Alarm, it will reapperar as a new alarm if the instrument value or the condition for the alarm has not become good.

When is an alarm triggered?

- An instrument reports an offrange value
- A maintenance prewarns
- A maintenance becomes due
- Robot Arm blocked or collision with another robot - See Operator's Quick help
- Alarm activation by Robot Parameter ax, Ax, A0 - See Messages with parameters from Fisa Robot

If the object of the alarm is a descendant to a position:

A basket present or a basket put in that position be marked with Remark.
If the object of the alarm is not a descendant to a position:

All baskets present in positions being descendants to the object will be marked with Remark.

To avoid having all baskets marked by an object at Installation level, uncheck the following submenu:
Mark Baskets for Global Alarms
You find it under menu Alarms
Visual indication

| A marked basket will change its backcolor to light red. |

See also Basket Colors and Properties
Alarm Types

- Generic - Alarm activation by Robot Parameter - A0
- Prewarn - Maintenance
- Due - Maintenance
- Exceeding - Instrument
- Insufficient - Instrument
- No Value - Instrument
- Maximum process residence time in position exceeded - Basket
- Minimum process residence time in position not respected - Basket
- Output - Alarm activation by Robot Parameter - Ax: x = 1 - 64
- Position - Alarm activation by Robot Parameter - ax: x = 1 - 65
- Failed - Alarm activation by Robot Parameter - Ax: x = 1 - 64
- Arm Blocked - Alarm activation by Robot Programming Unit