Ausgangsanschlüsse |

How to add and remove connections
Left panel
Right panel
Bottom panel
Wie wird eine Ausgang-Verbindung geändert
Vorgang
Rückmeldungs-Objekt
Siehe auch
Eingangsanschlüsse
Standardverbindungen für Ausgänge, Eingänge und Rückmelde-Objekte

This window is reached from the Program menu, Physical Output Connections submenu.

How to add and remove connections

The connection window has three panels:

- Left panel
- Right panel
- Bottom panel Zum verbinden
  Expand the tree by clicking on the '+' symbol.
  You select an Output in the Left panel and an Accessory in the Right panel.
  Click on the Connect button.
  The connection is added to the list in the Bottom panel. Um eine Verbindung zu trennen:
  Select a connection in the Bottom panel.
  Click the Remove button.
  Left panel

  Displays a tree containing all outputs that can be connected: Nur die physicalische Ausgänge können angeschlossen werden Configuration of Outputs and Inputs in the Programming Unit

  Local Physical are shown in black.
  Common Physical are shown in red (External IO Modules)

  Angeschlossene Ausgänge werden in fetter Schreibweise angezeigt.
  Right panel

  Displays a tree showing all items that can be connected:

  Any Accessory can be connected and are marked with a screwdriver.
  Items that cannot be connected are marked with a crossed screwdriver.

  Angeschlossenes Zubehör ist in fetter Schreibweise angezeigt.
  Bottom panel

  Displays a list containing all the connections made. Clicking on any connection will select the Output in the left panel and the Accessory in the right panel.

  The checkbox on the left of any connection can be unchecked if you do not want activations of the output to be registered in the database. Datenbank, wo Daten gespeichert sind
  Wie wird eine Ausgang-Verbindung geändert

  An Output connection has an Action property.
  It can also have an Response Object.
  Vorgang

  The third column in the Connections list contains the Action property. This property is necessary for the Automatic Program. See also Standardverbindungen

  Double-click on the connection to edit the Action property.

  | Aktivierung Deaktivierung Öffnen Schließen Aufwärts Abwärtshub Motor, Kettenförderer Zutritt Erlaubniß Verbindung zum Eingang

  You can also add a user defined Action. Menu User

  Removing the Action property excludes the connection from the Automatic Program.
  Rückmeldungs-Objekt

  The Output in the leftmost column in the Connections list can be bold and green. Beispiel:
  Robot A, Output 2

  This indicates that the Connection has an Response Object. The Response Object is necessary for testing the Robot program in Simulation Mode.
  Right-click on he connection to gain access to the popup menu:

  Here you can Add or Edit the Response Object. Rückmeldungs-Objekt