Berechnung der Zykluszeit |

Wie wird die Zykluszeit definiert?
Wie wird die Zykluszeit berechnet?
Columns in Cycle Time Window
Wie wird die Zykluszeit definiert?

Cycle time is defined as the time elapsed between two baskets exiting the line when the line is fully loaded. This time is normally somewhat longer than the longest minimum residence time. The extra time is accounted for by robot movements, lids opening, etc.

Wie wird die Zykluszeit berechnet?

The cycle time is typically calculated for the basket sequence taking the longest time. In a line with more than one robot, each robot will have its own cycle time. The cycle time for the basket sequence will never be shorter than that of the longest robot cycle time. Ideally, the cycle times of the robots should be equal, giving the cycle time of the basket sequence in question. The cycle time calculation must be performed for one robot at a time. This can be done by creating installations that are the relevant fragments for each robot. Thus, it is possible to correct the basket sequence if any bottlenecks are identified. When bottlenecks have been reduced to a minimum, a full simulation will give the best approximation of cycle time for the basket sequence.

Columns in Cycle Time Window

Korb | Der Korb, für den die Zykluszeit berechnet war.
| Total | Gesamte Zykluszeit Wait until the Corr value is 0 (zero) or that the Total Cycle Time has stabilized.
| Move X | Gesamtzeit der X-Bewegungen
| Move Y | Gesamtzeit der Y-Bewegungen
| Wait T | Gesamtzeit warten auf Timer
| Wait I | Gesamtzeit warten auf Eingänge
| Pause | Gesamtzeit der Pausen
| Idle | Gesamtzeit für andere Instruktionen
| Corr | Correction for graphical movements Graphics, in average, are NOT finished before the calculated time for robot movements. This correction is self-adjusting after each cycle. Wait until the Corr value is 0 (zero) or that the Total Cycle Time has stabilized.
| Count | Total instructions performed for the basket. This count can vary by one or two depending on round-offs of timers.
|