Rückmeldungs-Objekt |

What does it do?
Default Response Object
User defined Response Object
Parameter
Response Object Explained
What does it do?

The Response Object is necessary for testing the Robot program in Simulation Mode. It activates/inactivates an associated input as an answer to activation/inactivation of an output.

Verbundener Eingang | The number of the input (local or common)
Zeit für Rückmeldung (sekunden) | Number of seconds for delaying the response on the associated input. Default response times can be set by the user: Ansprechzeit der Deckel Externe Lift Out-Zeit Externe Lift Out Verweilzeit Kettenvorschubzeit Menü Simulation
Invertierte Rückmeldung | If checked, the response (after elapsed time for response) of the associated input will be the opposite of the output.
Sofortige invertierte Rückmeldung | If not checked, the status of the associated input will remain unchanged during the delay. If checked, the status will be immediately forced to the opposite of the expected response. After the response time is elapsed the associated input will be activated or deactivated depending on the setting in Inverted Response.
Eingang-Rückmeldung für OL | If checked, the associated input will be affected by activation of the Output.
Eingang-Rückmeldung für OH | If checked, the associated input will be affected by inactivation of the Output.
Robot B, Output 2, Upstroke: External Liftout, Tank 6 | Description (or name) of the Response Object It can be changed by the user. It also appears in the Structure Report. Anlagenstruktur

Response Object Explained