Instrumente |

Instrument Interface
Aktuelles Wert
Einheit
Minimum
Set value
Maximum
Welche Werte werden angezeigt
Wert unter min
Wert zwischen min und max
Wert über max
Instrument Popup Menu
Here you can set the Instrument number.
A number of individual display options are available.
Instrumenten-Gruppe
Important Observation

Siehe auch
Menü Instrumente
Instrumente auflisten
Instrument Interface

| There are five areas you can click on (left-click) to let you change settings for the instrument:

1. Aktuelles Wert ( Grau ) Enabled only if the instrument is manual.
2. Einheit ( Blau ) Siehe Einheiten
3. Minimum ( Gelb )
4. Set value ( Grün )
5. Maximum ( Rot )

Welche Werte werden angezeigt

| Wert unter min

| Wert zwischen min und max

| Wert über max

Instrument Popup Menu

| With a right-click on the instrument you reach more features than by clicking on it. Here you can set the Instrument number. A number of individual display options are available.

Instrumenten-Gruppe

If only one Instrument Family is defined (normal case) clicking on the menu will have no effect. If more than one Instrument families have been defined, you can choose family from the window that is displayed.

Important Observation

Any settings on the instruments in the Fisa Project interface do not have any influence on the real instruments. Settings such as Min and Max only serve to trigger critical process events in Fisa Logger (and Simulation). Fisa Logger

For example, if a physical instrument is configured to report temperature in degrees Celsius, changing the unit to degrees Farenheit in Fisa Project will have no effect on the physical instrument. The Fisa Logger will receive values from the physical instrument in degrees Celsius but Fisa Logger will report the values in unit Fahrenheit!

When using Fisa Logger ensure that the instrument definitions are coherent with physical instrument settings. This applies to Unit and Instrument Number. You can still use your own Min and Max values to trigger critical process events in Fisa Logger.

The physical instruments are configured from the factory.
Any modifications to the original settings are performed separately.