Menü Simulation |

Introduktion
Rückmeldungs-Objekte erstellen
Alle Rückmeldungs-Objekte entfernen
Rotationszeit
Ansprechzeit der Deckel
Externe Lift Out-Zeit
Externe Lift Out Verweilzeit
Kettenvorschubzeit
Koordinaten-Auflistung
Berechnung der Zykluszeit
Korbbericht (kurz)
Simuliere TR 2000-Programm
Berechnete Bewegungsgeschwindigkeit verwenden

Introduktion

| Simulation is started by clicking on the submenu Simuliere TR 2000-Programm (Ctrl + S) In simulation mode, baskets are blue.

The testing is carried out in simulation mode running a robots program file. The instructions in the program are carried out independently for each robot. By using the predefined Response Objects the status of inputs can be simulated. The status of inputs can also be set manually by using the IO window for any virtual programming unit.

Sehen Sie auch:
Rückmeldungs-Objekte erstellen

Alle Rückmeldungs-Objekte entfernen

| You will have to set the inputs manually while simulating.

Rotationszeit

Enabled for Robots with Rotation Grip.
Ansprechzeit der Deckel

| This is the default response time for inputs connected to the lid opened/closed detector switches. You can change this value individually for each response object.

Externe Lift Out-Zeit

| This is the default response time for the input connected to the external liftout high position signal. You can change this value individually for each response object.

Externe Lift Out Verweilzeit

| This is the default time for starting the liftout sequence after enabling upstroke on the liftout. You can change this value individually for each response object.

Kettenvorschubzeit

| This is the default time for a complete turn of the chain gearwheel. A detector switch detects when the wheel is in step position. You can change this value individually for each response object.

Koordinaten-Auflistung

This is used only for estimating the cycle time.
Siehe Koordinaten-Auflistung
Berechnung der Zykluszeit

Siehe Berechnung der Zykluszeit
Korbbericht (kurz)

Siehe Korbbericht (kurz)
Simuliere TR 2000-Programm

Asks for program to load and starts Simulation Mode
Berechnete Bewegungsgeschwindigkeit verwenden

When this menu is checked the graphics will move with 'real' robot speed (Normalerweise langsamer als die Geschwindigkeit in der Simulation)